IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "e:/temp/worker_COMMON_8338/temp/tmp_7504_1_Oxqmc/format_2/GL------.01000H0200S0083S0083AN-03AABEBBAAE.---------.A00033Z1-Z----.-------.--.ifc"
Time stamp: "2026-05-27T06:14:51"
Originating system: "PARTsolutions"
Application: "PARTsolutions" version "V12.0" identifier "PARTsolutions" by Organization "Cadenas"

People and organizations
  Person "Cadenas" of Organization "Cadenas"
  Owner history of Person "Cadenas" of Organization "Cadenas" | application "PARTsolutions" version "V12.0" identifier "PARTsolutions" by Organization "Cadenas" | change ADDED | created 1779862486 (2026-05-27T06:14:46Z) | last modified 1779862486 (2026-05-27T06:14:46Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  SOLIDANGLEUNIT: STERADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND

Spatial structure
IFCPROJECT "GL------.01000H0200S0083S0083AN-03AABEBBAAE.---------.A00033Z1-Z----.-------.--" | description "Straight Belt Conveyors"
  IFCBUILDING "BUILDING"
    contains 1 element
      1 x IFCDISCRETEACCESSORY | names: "GL------.01000H0200S0083S0083AN-03AABEBBAAE.---------.A00033Z1-Z----.-------.--" | descriptions: "GL------.01000H0200S0083S0083AN-03AABEBBAAE.---------.A00033Z1-Z----.-------.--" | property sets: Pset_ManufacturerTypeInformation, ePset_PARTsolutions

Property sets
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCDISCRETEACCESSORY)
    ArticleNumber = "GL------.01000H0200S0083S0083AN-03AABEBBAAE.---------.A00033Z1-Z----.-------.--" (IFCIDENTIFIER)
    Manufacturer = "MTF" (IFCLABEL)
  ePset_PARTsolutions | properties | on 1 object (1 IFCDISCRETEACCESSORY)
    ABH = "83" (IFCTEXT)
    AD = "ja" (IFCTEXT)
    AN = "ja" (IFCTEXT)
    ANTRIEB = "Außenliegender Antrieb (Standard)" (IFCTEXT)
    ANTRIEBPOS = "1 : ziehend, Bandauslauf, links (Standard)" (IFCTEXT)
    ANTRIEBST = "N/A" (IFCTEXT)
    ASPANN = "400 V" (IFCTEXT)
    AUFB = "N/A" (IFCTEXT)
    AUH = "83" (IFCTEXT)
    BANDBE = "" (IFCTEXT)
    BETRIEB = "konstant (Standard)" (IFCTEXT)
    BG = "3.3" (IFCTEXT)
    BNEB = "200" (IFCTEXT)
    BNEL = "1000" (IFCTEXT)
    BNUB = "200" (IFCTEXT)
    BSTG = "0" (IFCTEXT)
    CATALOG = "MTF Technik" (IFCTEXT)
    FDA = "nein" (IFCTEXT)
    FOEBES = "" (IFCTEXT)
    FRICHT = "zum Bandauslauf hin (Standard)" (IFCTEXT)
    GURTAUS = "Standardauswahl" (IFCTEXT)
    GURTBES = "Gurt-Nr. 3: min. Umlenkung Ø30mm; Temperaturbereich von -10°C bis +80°C; nicht FDA-konform; bedingt öl- und fettbeständig; Tragseitenmaterial aus PVC mit glatter, glänzender Oberfläche; adhäsiv; antistatisch; petrol; Gurtdicke ca. 2,0 mm; keine Abschälung; I; mögl. Stollen: TR, R, T, TN, SO, SG, SY60, SY70;" (IFCTEXT)
    GURTD = "2.0" (IFCTEXT)
    GURTFARB = "petrol" (IFCTEXT)
    GURTINFO = "Weitere Informationen zu den Gurten" (IFCTEXT)
    GURTMAT = "PVC" (IFCTEXT)
    GURTNR = "3 (Standard)" (IFCTEXT)
    GURTOBER = "glatt [glänzend]" (IFCTEXT)
    INDEX = "I" (IFCTEXT)
    INFO = "Weitere Informationen zu dem Multi-Tech Gurtförderer Typ GL" (IFCTEXT)
    LINA = "GL------.01000H0200S0083S0083AN-03AABEBBAAE.---------.A00033Z1-Z----.-------.--" (IFCTEXT)
    MAXBANDBE = "7.0" (IFCTEXT)
    MFABSTAND = "0" (IFCTEXT)
    MU = "Ø 80" (IFCTEXT)
    NB = "GL------.01000H0200S0083S0083AN-03AABEBBAAE.---------.A00033Z1-Z----.-------.--" (IFCTEXT)
    NBSYN = "$CNSORDERNO." (IFCTEXT)
    NN = "Type GL" (IFCTEXT)
    NT = "Gerades Förderband mit Laufdecke" (IFCTEXT)
    OI = "bedingt" (IFCTEXT)
    PROJBEZ = "" (IFCTEXT)
    QUERKR = "nein" (IFCTEXT)
    SFH = "GL 0" (IFCTEXT)
    STAB = "0" (IFCTEXT)
    STABMIN = "0" (IFCTEXT)
    STANZ = "0" (IFCTEXT)
    STAUS = "Ohne" (IFCTEXT)
    STF = "Ohne" (IFCTEXT)
    STFARBE = "N/A" (IFCTEXT)
    STH = "0" (IFCTEXT)
    STM = "Ohne" (IFCTEXT)
    TEMPMAX = "80" (IFCTEXT)
    TYP = "Waagerechte Förderbänder" (IFCTEXT)
    UANZ = "0" (IFCTEXT)
    UAUS = "ohne" (IFCTEXT)
    UBV = "N/A" (IFCTEXT)
    ULA = "Umlenkung Ø 80 (Standard)" (IFCTEXT)
    ULE = "Umlenkung Ø 80 (Standard)" (IFCTEXT)
    URB = "0" (IFCTEXT)
    UTYP = "N/A" (IFCTEXT)